* ARQ instead of FEC for resending original packet instead of correcting it with FEC
  + Stop-and-Wait ARQ, if too slow then maybe >>> Go-back-N ARQ (multiple packets does not have to wait for ack after every)
* CRC32() from zlib for verifying integrity

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| TYPE | SEQ Nr. | Frag. Nr | Total Frags | CRC | Flags | Data |
| 1B | 4B | 2B | 2B | 4B | 1B |  |